{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["KI-Part-ist"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"KI-Part-ist","index":0,"n_rows":12,"n_cols":8,"rows_kept":12,"cut":false,"hidden":false,"merged":[[1,1,1,7]],"flags":["formulas_cached_only"]}
[]
[null,"Przedmiar robót  -     budowa ul. Partyzantów -  odcinek istniejący - chodniki"]
[null,"Numer","Podstawa","Opis","Jednostka","Ilość","Cena jedn.","Wartość"]
[null,"4","Element","Roboty brukarskie"]
[null,"4.1"]
[null,"4.2","KNNR 6/0404-0500","Obrzeża betonowe prostokątne i łukowe o wymiarach 30x8 cm, posadowione na ławie wraz z oporem - z betonu B10 ","m",206]
[null,"4.3","KNNR 6/0106-0200","Warstwy odcinające z piasku zagęszczane ręcznie, grubość warstwy 10 cm","m2",466.5]
[null,"4.4"]
[null,"4.5","KNNR 6/0502-0201","Chodniki z kostki brukowej betonowej kolorowej typ Nostalit grubości 6 cm, układany na stabilizacji \"75\"    (  75 kg cementu na 1m3 piasku ).","m2",466.5]
[null,"4.6"]
[null,null,null,"Razem netto:"]
[null,null,null,"Razem z VAT:"]