{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Arkusz1","Arkusz2","Arkusz3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Arkusz1","index":0,"n_rows":10,"n_cols":7,"rows_kept":10,"cut":false,"hidden":false,"merged":[[3,1,3,6]],"flags":["formulas_cached_only"]}
[]
[]
[]
[null,"PRZEDMIAR ROBÓT                                                          Remont drogi gminnej nr V/6  w msc. Łęg, gmina Połaniec"]
[null,"Lp.","Wyszczególnienie","Zakres robót","Jednostka miary","cena jednostkowa w złotych","Wartość robór w złotych brutto"]
[null,"1.","Poprawienie profilu drogi równiarką 3mx332m=996m2 + 4m2",1000,"m2"]
[null,"2.","Wykonanie podbudowy tłuczniowej z kamienia dolomitowego frakcja 4/31,5mm ,śr. gr. 8cm wraz z wyprofilowaniem równarką, zaklinowaniem oraz zagęszczeniem walcem",1000,"m2"]
[null,"3.","Warstwa profilująca z masy min.-asfaltowej gr.5cm",1000,"m2"]
[null,"4.","Pobocza dwustronne z rumosza śr gr.5cm - 2x0,5mx332m=332m",332,"m2"]
[null,null,"Suma całego zadania"]

{"sheet":"Arkusz2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Arkusz3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}