{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Arkusz1","Arkusz2","Arkusz3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Arkusz1","index":0,"n_rows":18,"n_cols":7,"rows_kept":18,"cut":false,"hidden":false,"merged":[[7,1,7,6],[3,1,3,6]],"flags":["formulas_cached_only"]}
[]
[]
[]
[null,"PRZEDMIAR ROBÓT"]
[]
[]
[]
[null," Remont drogi gminnej nr 364124T w Ruszczy na terenie gminy Połaniec"]
[]
[null,"Lp.","Wyszczególnienie","Jednostka","Zakres ","Cena za jednostkę zł brutto","Wartość brutto zł"]
[null,"1.","Prace pomiarowe przy robotach ziemnych, dla trasy drogowej wraz z wytyczeniem i operatem geodezyjnym powykonawczym.","mb",1396]
[null,"2.","Profilowanie równiarką drogi z zebraniem przerostu trawy i wywozem urobku na odległość do 10km -  pow. 1396mx3,0m=4188m2 +150m2=4338m2","m2",4338]
[null,"4.","Wykonanie podbudowy tłuczniowej z dolomitu fr. 4-63mm gr. 10cm stabilizowanej mechanicznie z zakinowaniem  -  pow.1396mx3,0m=4188m2 +150m2=4338m2","m2",4338]
[null,"5.","Wykonanie w-wy ścieralnej z masy min.-asfalt. po zagęszczeniu gr.4cm - pow. 1396mx3,0m=4188m2 +150m2=4338m2","m2",4338]
[null,"6.","Pobocze z klińca dolomitowego śr. gr. 8cm szer. 2x0,5x1396m*0,08m=111,68m3","m3",111.68]
[null,"7.","Odmulenie rowu gł. 20cm z wywiezieniem urobku na odległość do 10km dł. 180mb","mb",180]
[null,"8.","Ustawienie znaku drogowego A-7","szt.",2]
[null,null,"Razem"]

{"sheet":"Arkusz2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Arkusz3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}