{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Arkusz1","Arkusz2","Arkusz3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Arkusz1","index":0,"n_rows":39,"n_cols":7,"rows_kept":39,"cut":false,"hidden":false,"merged":[[2,1,2,6],[6,1,6,6],[31,1,31,6],[4,1,4,6]],"flags":["formulas_cached_only"]}
[]
[]
[null,"                                                                            Załącznik nr 1C"]
[]
[null,"PRZEDMIAR ROBÓT"]
[]
[null,"Budowa drogi gminnej - łącznik ul Sportowa z ul. Reymonta w Połańcu"]
[]
[null,"Lp.","Wyszczególnienie","Jednostka","Zakres ","Cena za jednostkę zł brutto","Wartość brutto zł"]
[null,"1.","Prace pomiarowe przy robotach ziemnych, dla trasy drogowej wraz z wytyczeniem i operatem geodezyjnym powykonawczym","mb",173]
[null,"2.","Poprawienie istniejącego profilu drogi kruszywem dolomitowym fr. 4-31,5mm gr. 5cm - pow. 1290m2","m2",1290]
[null,"3.","Wykonanie w-wy profilującej z masy min.-asfalt. gr.4cm - pow. 1290m2","m2",1290]
[null,"4.","Wykonanie w-wy ścieralnej z masy min.-asfalt. gr.4cm - pow. 1290m2","m2",1290]
[null,"5.","Regulacja wpustów ulicznych","szt.",3]
[null,"6.","Regulacja studni kanalizacji ","szt.",3]
[null,null,"Razem"]
{"$rows_empty":15}
[null,"Zestawienie załączników "]
[]
[]
[null,"Lp.","Wyszczególnienie","Jednostka","Zakres ","Cena za jednostkę zł brutto","Wartość brutto zł"]
[null,"1.","Załącznik nr 1"]
[null,"2.","Załącznik nr 2"]
[null,"3.","Załącznik nr 3"]
[null,null,"Razem"]

{"sheet":"Arkusz2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Arkusz3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}