{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Zakres-2010"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Zakres-2010","index":0,"n_rows":15,"n_cols":8,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
[null,null,"Zakres robót do umowy TI.271.38.2014.ID-1","Gmina",null,null,"zał. nr 1"]
[null,null,"REMONT  CZĄSTKOWY DRÓG  PO  ZIMIE    -   MiG POŁANIEC  2014 rok"]
[]
[null,"lp","OPIS","jednostka","ilość jedno","cena jed. brutto","Razem PLN","Uwagi"]
[null,1,"Remont cząstkowy dróg przy użyciu ciśnieniowego urzadzenia tzw. remontera o gr. od 2-4 cm emulsja asfaltową.","m2",600]
[null,2,"Wykonanie remontu cząstkowego masą min.-asfaltową o gr. śr. 4 cm z obcięciem krawedzi wyboju i posmarowaniem emulsja asfaltową.","m2",25]
[null,3,"Regulacja  studzienek i włazów  betonem B-20","szt",5]
[null,4,"Uzupełnienie poboczy klińcem kamiennym dolomitowym gr. 6 cm wraz z wyprofilowaniem i zageszczeniem","m2",120]
[]
[]
[null,null,"OGÓŁEM:","x",null,"x",0,"x"]
[]
[]
[null,null,"Cena zawiera 23% podatek VAT"]